**For Immediate Release:** May 2025

**NEW! Reedy Power RX/Servo Y-Connector 95mm, Black**

Reedy Power, a leader in [high-performance RC electronics](https://x.com/i/grok?text=high-performance%20RC%20electronics), proudly introduces the latest addition to their product lineup, a 95mm Y-Connector.



**Key Features Include:**

* [**Universal Compatibility**](https://x.com/i/grok?text=Universal%20Compatibility)**:** The new Y-connector lead is compatible with a wide range of RC vehicles, ensuring that it can be used with your existing setup, whether you're into on-road, off-road, rock crawling, boats, or aircraft.
* **High-Quality Construction:** Crafted with precision, the Y-connector features [low-resistance connectors](https://x.com/i/grok?text=gold-plated%20connectors) for superior conductivity and resistance to corrosion. Durable insulation ensures reliability and longevity.
* [**Dual Servo Control**](https://x.com/i/grok?text=Dual%20Servo%20Control)**:** This Y-connector allows for the connection of two servos to a single channel on your receiver, perfect for applications requiring synchronized servo operation, like steering or dual throttle setups.
* **Optimal Signal Integrity:** Engineered to maintain [signal integrity](https://x.com/i/grok?text=signal%20integrity), the Y-connector reduces the risk of interference, providing smooth and precise control even in the most demanding conditions.
* [**Easy Installation**](https://x.com/i/grok?text=Easy%20Installation)**:** With a cable length of 95mm, this lead offers enough reach to connect comfortably without clutter and includes + - S markings for easy polarity identification.

**Applications:**

* **ESC Programming:** Provides Fan and Programmer connection options where only a single port is shared for both.
* [**Dual Servo Setups**](https://x.com/i/grok?text=Dual%20Servo%20Setups%20in%20Rock%20Crawlers)**:** Allows dual servo operation from a single channel.
* [**Aircraft Control Surfaces**](https://x.com/i/grok?text=Aircraft%20Control%20Surfaces)**:** Where dual servos on a single control surface are used for increased torque or redundancy.

The Reedy Power 95mm Y-Connector Lead is now available online at [www.reedypower.com](http://www.reedypower.com/), or at your favorite hobby retailer.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **UPC** | **Part No.** | **Description** | **MSRP** | **MAP** | **COO** | **Available** |
| 784695271708 | 27170 | Reedy Power RX/Servo Y-Connector 95mm, black | $6.99 | $6.99 | CN | button-buy-now-200px |